Kensington sd3000v/sd3500v USB 3.0 docking stations (K33970/K33971/K33972/K33973) 
and K33928 Video Adapter Software Driver Version 7.0.43577.0

A. Introduction
===============
This Software Release delivers the following features:
- Windows 8 support
- Wake on LAN support for sd300v and sd3500v products
- Configurable MAC address for sd300v and sd3500v products
- VLAN support for sd300v and sd3500v products
- Critical bug fixes and compatibility improvements for all products

Corporations can apply for a corporate install version at 
www.displaylink.com/corporateinstall


B. Supported Kensington Products
================================

This software driver was designed for the following products:

1) sd3000v/sd3500v USB 3.0 docking stations (K33970/1/2/3)
2) K33928 Universal Display Adapter

C. Supported Operating Systems
==============================
This release can be installed on the following operating systems:

    - Windows XP SP1 (32-bit edition only)
    - Windows XP SP2 (32-bit edition only)
    - Windows XP SP3 (32-bit edition only)
    - Windows Vista SP1 (32-bit and 64-bit editions)
    - Windows Vista SP2 (32-bit and 64-bit editions)
    - Windows 7 (32-bit and 64-bit editions)
    - Windows 8 (32-bit and 64-bit editions)

Video: video is supported in extend mode with most popular video players on
Windows XP and Windows 7/Vista in WDDM/Aero Mode. Video support is limited in
other configurations including mirror mode and Windows 7/Vista Basic Mode.


D. How to Install and use
=========================
Please find detailed guidance and information about how to install and use this
software in the DisplayLink Software User Guide: http://kb.displaylink.com/298

Corporations can apply for a corporate install version at 
www.displaylink.com/corporateinstall

For further support and information about DisplayLink software, please visit 
http://www.displaylink.com/support


D. Known Issues and Limitations
===============================

System behaviour with USB Docking station or USB Display Adapter attached screens has been well tested.
Testing covers plug/unplug, mode changes, playing video, hibernate,sleep/standby, multiple users, different user rights, attached screen as primary screen, attached screen as only screen, and other aspects.

Some use cases my exhibit minor issues, general troubleshooting recommendations
are:
    - detach then reattach the USB docking station or USB Display Adapter's USB cable
    - change display settings using USB display adapter GUI (Vista only)  
    - change display settings using WDP.
    - ensure you have the latest graphics drivers installed for your system GPU.

E.Requirements:
===============

    - At least one USB 2.0 port
    - 30 megabytes (MB) of free disk space
    - External computer screen

PC Recommended Specifications:
------------------------------
    - The software driver can be run on PCs ranging from Netbooks, Notebooks/Laptops, and Desktops - on processors ranging from Atom N270 based PCs, basic single Core CPUs, and of course the latest Dual and Quad Core CPUs.
    - The USB video screens are not supported on systems with two graphics cards used simultaneously (supporting separate screens, or in ATI Crossfire configuration). Two graphics cards in Nvidia SLI configuration are supported but not on Windows 7.
    - The performance of the software is dependent upon the processing power available, and so more capable systems offer higher performance.

Recommended typical system requirements are:
-------------------------------------------- 
- Windows® 8/7/Vista:
-------------------
For Windows® Vista, the Windows Experience Index (WEI) is a useful measure of hardware level. The WEI is accessible from Computer->Properties or from Control Panel->System.
For more information please visit http://windowshelp.microsoft.com/windows/en-us/help/0fee4637-8b21-41f1-87f6-66d2205420d61033.mspx
The recommended typical hardware requirements for the PC are
    - WEI score of at least 3.0 in the 'Graphics; Desktop performance for Windows Aero' category.
    - Recommended: WEI score of at least 3.0 overall, as recommended by Microsoft.
    - For full-screen video playback the recommended hardware depends on the display resolution: 
        -- 1366x768: overall WEI score of at least 3.5
        -- 1920x1080 (HD): overall WEI score of at least 4.0 and a modern GPU (GPU introduced to the market after 2H'08 or top-of-the-line GPU introduced in 2008).
    - At least one USB 2.0 port.
    - 30 megabytes (MB) of free disk space.
    - Computer screen for use with the USB Display device, if it is not integrated.
    - Network access for software downloads, or access to a CD-ROM drive.
    - If the PC specification is below this, performance will be lower (or CPU loading higher).

- Windows® XP:
--------------
    - For 1-2 monitors, business usage, productivity target. This may not provide full frame rate DVD playback at full screen. 
    - 1.2GHz Single Core CPU (Celeron or Atom N270 for example)
    - 512MB memory
    - For 3 monitors where 1 could run DVD video while also targeting productivity and business apps. Will support only 1 video of DVD resolution at full screen: 
         - 1.6GHz CPU
         - 1GB memory
    - For 6 screens where 1 screen can run full screen DVD video: 
         - 1.8GHz Core Duo
         - 1GB memory

F. Installation and Operation Instructions
==========================================

To install the SW driver, unzip the downloaded "K33970-1-2-3_DRV_7.0.43577.0.zip" into a local folder and then double click "setup.exe" and follow the on screen instructions.

Visit http://expandyourworkspace.kensington.com for detailed operation instructions.